**Lab 12 Notes: Interrupts**

**Key Terms**

* **Trigger**: A hardware event (the automatic transfer of software execution to a hardware event; an interrupt)
* **Process**: is the action of software as it executes
* **Thread**: The path of action a software takes as it is executed
  + **Background thread**: The execution of the interrupt service routine
  + **Foreground thread**:
  + **Multi-threaded**: foreground and background threads cooperating to perform an overall task.
* **EnableInterupts():** Allows interrupts to happen at this time
  + PRIMASK = 0
* **DisableInterupts():** Postpone interrupts until a later time.
  + PRIMASK = 1
* **PRIMASK:** Interrupt Priority Mask
* **BASEPRI**: Is a register for setting interrupt priority.
  + If BASEPRI is set to 3, requests level 0,1, and 2 can interrupt. Anything above 3 will be postponed. If BASEPRI is set to 0 then nothing can interrupt the current interrupt.
* **Context switch:** The steps an interrupt process routine goes through switching from **foreground** thread to a **background** thread, or when going from lower priority thread to higher priority thread.
* **LR:** (Link Register) holds the address to return to when a function call completes.
* **PC:** (Program Counter)
* **IPSR:** (Interrupt program status register)
* **ISR:** (Interrupt service routine)

**Conditions for Interrupts to be executed:**

1. **Device is armed** – Allow the hardware trigger to interrupt.
2. **NVIC is enabled for the device** – Set the NVIC enable bit under 0xE000.E100 NVIC register.
3. **EnableInterupts()** – the function will set PRIMASK = 0.
4. **Has priority** – BASEPRI is set higher than the current running interrupt.
5. **Trigger** – The external hardware event that will trigger the interrupt becomes active/true

**Interrupt process routine (the context switch):**

1. Finish processing the current instruction when an interrupt trigger occurs
2. Push registers R0, R1, R2, R3, R12, R13 (Link Register), Program Counter, and Processor Status Register to the stack (a special region in memory that stores temporary variables created by functions() --- including main() function).
3. Link register (LR) is set to 0xFFFF.FFF9
4. Interrupt Program Status Register (IPSR) is set to the interrupt number being processed.
5. Program Counter (PC) is loaded with the interrupt vector (address of the ISR vector).